Crypto++ 8.6 Free C++ class library of cryptographic schemes

cpu.h
Go to the documentation of this file.
1 // cpu.h - originally written and placed in the public domain by Wei Dai
2 // updated for ARM and PowerPC by Jeffrey Walton.
3 // updated to split CPU_Query() and CPU_Probe() by Jeffrey Walton.
4
5 /// \file cpu.h
6 /// \brief Functions for CPU features and intrinsics
7 /// \details The CPU functions are used in IA-32, ARM and PowerPC code paths. The
8 /// functions provide cpu specific feature testing on IA-32, ARM and PowerPC machines.
9 /// \details Feature detection uses CPUID on IA-32, like Intel and AMD. On other platforms
10 /// a two-part strategy is used. First, the library attempts to *Query* the OS for a feature,
11 /// like using Linux getauxval() or android_getCpuFeatures(). If that fails, then *Probe*
12 /// the cpu executing an instruction and an observe a SIGILL if unsupported. The general
13 /// pattern used by the library is:
14 /// <pre>
15 /// g_hasCRC32 = CPU_QueryCRC32() || CPU_ProbeCRC32();
16 /// g_hasPMULL = CPU_QueryPMULL() || CPU_ProbePMULL();
17 /// g_hasAES = CPU_QueryAES() || CPU_ProbeAES();
18 /// </pre>
19 /// \details Generally speaking, CPU_Query() is in the source file <tt>cpu.cpp</tt> because it
20 /// does not require special architectural flags. CPU_Probe() is in a source file that receives
21 /// architectural flags, like <tt>sse_simd.cpp</tt>, <tt>neon_simd.cpp</tt> and
22 /// <tt>ppc_simd.cpp</tt>. For example, compiling <tt>neon_simd.cpp</tt> on an ARM64 machine will
23 /// have <tt>-march=armv8-a</tt> applied during a compile to make the instruction set architecture
24 /// (ISA) available.
25 /// \details The cpu probes are expensive when compared to a standard OS feature query. The library
26 /// also avoids probes on Apple platforms because Apple's signal handling for SIGILLs appears to
27 /// corrupt memory. CPU_Probe() will unconditionally return false for Apple platforms. OpenSSL
28 /// experienced the same problem and moved away from SIGILL probes on Apple.
29
30 #ifndef CRYPTOPP_CPU_H
31 #define CRYPTOPP_CPU_H
32
33 #include "config.h"
34
35 // Issue 340
36 #if CRYPTOPP_GCC_DIAGNOSTIC_AVAILABLE
37 # pragma GCC diagnostic push
38 # pragma GCC diagnostic ignored "-Wconversion"
39 # pragma GCC diagnostic ignored "-Wsign-conversion"
40 #endif
41
42 // Applies to both X86/X32/X64 and ARM32/ARM64
43 #if defined(CRYPTOPP_LLVM_CLANG_VERSION) || defined(CRYPTOPP_APPLE_CLANG_VERSION)
44 #define NEW_LINE "\n"
45 #define INTEL_PREFIX ".intel_syntax;"
46 #define INTEL_NOPREFIX ".intel_syntax;"
47 #define ATT_PREFIX ".att_syntax;"
48 #define ATT_NOPREFIX ".att_syntax;"
49 #elif defined(__GNUC__)
50 #define NEW_LINE
51 #define INTEL_PREFIX ".intel_syntax prefix;"
52 #define INTEL_NOPREFIX ".intel_syntax noprefix;"
53 #define ATT_PREFIX ".att_syntax prefix;"
54 #define ATT_NOPREFIX ".att_syntax noprefix;"
55 #else
56 #define NEW_LINE
57 #define INTEL_PREFIX
58 #define INTEL_NOPREFIX
59 #define ATT_PREFIX
60 #define ATT_NOPREFIX
61 #endif
62
63 // Thanks to v1ne at https://github.com/weidai11/cryptopp/pull/1133
64 #define PERCENT_PASTE(x) "%" #x
65 #define PERCENT_REG(x) PERCENT_PASTE(x)
66
67 #ifdef CRYPTOPP_GENERATE_X64_MASM
68
69 #define CRYPTOPP_X86_ASM_AVAILABLE
70 #define CRYPTOPP_BOOL_X64 1
71 #define CRYPTOPP_SSE2_ASM_AVAILABLE 1
72 #define NAMESPACE_END
73
74 #else
75
76 NAMESPACE_BEGIN(CryptoPP)
77
78 // ***************************** IA-32 ***************************** //
79
80 #if CRYPTOPP_BOOL_X86 || CRYPTOPP_BOOL_X32 || CRYPTOPP_BOOL_X64 || CRYPTOPP_DOXYGEN_PROCESSING
81
82 #define CRYPTOPP_CPUID_AVAILABLE 1
83
84 // Hide from Doxygen
85 #ifndef CRYPTOPP_DOXYGEN_PROCESSING
86 // These should not be used directly
87 extern CRYPTOPP_DLL bool g_x86DetectionDone;
88 extern CRYPTOPP_DLL bool g_hasSSE2;
89 extern CRYPTOPP_DLL bool g_hasSSSE3;
90 extern CRYPTOPP_DLL bool g_hasSSE41;
91 extern CRYPTOPP_DLL bool g_hasSSE42;
92 extern CRYPTOPP_DLL bool g_hasMOVBE;
93 extern CRYPTOPP_DLL bool g_hasAESNI;
94 extern CRYPTOPP_DLL bool g_hasCLMUL;
95 extern CRYPTOPP_DLL bool g_hasAVX;
96 extern CRYPTOPP_DLL bool g_hasAVX2;
97 extern CRYPTOPP_DLL bool g_hasSHA;
98 extern CRYPTOPP_DLL bool g_hasADX;
99 extern CRYPTOPP_DLL bool g_isP4;
100 extern CRYPTOPP_DLL bool g_hasRDRAND;
101 extern CRYPTOPP_DLL bool g_hasRDSEED;
102 extern CRYPTOPP_DLL bool g_hasPadlockRNG;
103 extern CRYPTOPP_DLL bool g_hasPadlockACE;
104 extern CRYPTOPP_DLL bool g_hasPadlockACE2;
105 extern CRYPTOPP_DLL bool g_hasPadlockPHE;
106 extern CRYPTOPP_DLL bool g_hasPadlockPMM;
107 extern CRYPTOPP_DLL word32 g_cacheLineSize;
108
109 CRYPTOPP_DLL void CRYPTOPP_API DetectX86Features();
110 CRYPTOPP_DLL bool CRYPTOPP_API CpuId(word32 func, word32 subfunc, word32 output[4]);
111 #endif // CRYPTOPP_DOXYGEN_PROCESSING
112
113 /// \name IA-32 CPU FEATURES
114 //@{
115
116 /// \brief Determine SSE2 availability
117 /// \return true if SSE2 is determined to be available, false otherwise
118 /// \details MMX, SSE and SSE2 are core processor features for x86_64, and
119 /// the function return value is based on OSXSAVE. On i386 both
120 /// SSE2 and OSXSAVE are used for the return value.
121 /// \note This function is only available on Intel IA-32 platforms
122 inline bool HasSSE2()
123 {
124 #if (CRYPTOPP_SSE2_ASM_AVAILABLE || CRYPTOPP_SSE2_INTRIN_AVAILABLE)
125 if (!g_x86DetectionDone)
126 DetectX86Features();
127 return g_hasSSE2;
128 #else
129 return false;
130 #endif
131 }
132
133 /// \brief Determine SSSE3 availability
134 /// \return true if SSSE3 is determined to be available, false otherwise
135 /// \details HasSSSE3() is a runtime check performed using CPUID
136 /// \note This function is only available on Intel IA-32 platforms
137 inline bool HasSSSE3()
138 {
139 #if CRYPTOPP_SSSE3_AVAILABLE
140 if (!g_x86DetectionDone)
141 DetectX86Features();
142 return g_hasSSSE3;
143 #else
144 return false;
145 #endif
146 }
147
148 /// \brief Determine SSE4.1 availability
149 /// \return true if SSE4.1 is determined to be available, false otherwise
150 /// \details HasSSE41() is a runtime check performed using CPUID
151 /// \note This function is only available on Intel IA-32 platforms
152 inline bool HasSSE41()
153 {
154 #if CRYPTOPP_SSE41_AVAILABLE
155 if (!g_x86DetectionDone)
156 DetectX86Features();
157 return g_hasSSE41;
158 #else
159 return false;
160 #endif
161 }
162
163 /// \brief Determine SSE4.2 availability
164 /// \return true if SSE4.2 is determined to be available, false otherwise
165 /// \details HasSSE42() is a runtime check performed using CPUID
166 /// \note This function is only available on Intel IA-32 platforms
167 inline bool HasSSE42()
168 {
169 #if CRYPTOPP_SSE42_AVAILABLE
170 if (!g_x86DetectionDone)
171 DetectX86Features();
172 return g_hasSSE42;
173 #else
174 return false;
175 #endif
176 }
177
178 /// \brief Determine MOVBE availability
179 /// \return true if MOVBE is determined to be available, false otherwise
180 /// \details HasMOVBE() is a runtime check performed using CPUID
181 /// \since Crypto++ 8.3
182 /// \note This function is only available on Intel IA-32 platforms
183 inline bool HasMOVBE()
184 {
185 #if CRYPTOPP_SSE42_AVAILABLE
186 if (!g_x86DetectionDone)
187 DetectX86Features();
188 return g_hasMOVBE;
189 #else
190 return false;
191 #endif
192 }
193
194 /// \brief Determine AES-NI availability
195 /// \return true if AES-NI is determined to be available, false otherwise
196 /// \details HasAESNI() is a runtime check performed using CPUID
197 /// \since Crypto++ 5.6.1
198 /// \note This function is only available on Intel IA-32 platforms
199 inline bool HasAESNI()
200 {
201 #if CRYPTOPP_AESNI_AVAILABLE
202 if (!g_x86DetectionDone)
203 DetectX86Features();
204 return g_hasAESNI;
205 #else
206 return false;
207 #endif
208 }
209
210 /// \brief Determine Carryless Multiply availability
211 /// \return true if pclmulqdq is determined to be available, false otherwise
212 /// \details HasCLMUL() is a runtime check performed using CPUID
213 /// \since Crypto++ 5.6.1
214 /// \note This function is only available on Intel IA-32 platforms
215 inline bool HasCLMUL()
216 {
217 #if CRYPTOPP_CLMUL_AVAILABLE
218 if (!g_x86DetectionDone)
219 DetectX86Features();
220 return g_hasCLMUL;
221 #else
222 return false;
223 #endif
224 }
225
226 /// \brief Determine SHA availability
227 /// \return true if SHA is determined to be available, false otherwise
228 /// \details HasSHA() is a runtime check performed using CPUID
229 /// \since Crypto++ 6.0
230 /// \note This function is only available on Intel IA-32 platforms
231 inline bool HasSHA()
232 {
233 #if CRYPTOPP_SHANI_AVAILABLE
234 if (!g_x86DetectionDone)
235 DetectX86Features();
236 return g_hasSHA;
237 #else
238 return false;
239 #endif
240 }
241
242 /// \brief Determine ADX availability
243 /// \return true if ADX is determined to be available, false otherwise
244 /// \details HasADX() is a runtime check performed using CPUID
245 /// \since Crypto++ 7.0
246 /// \note This function is only available on Intel IA-32 platforms
247 inline bool HasADX()
248 {
249 #if CRYPTOPP_ADX_AVAILABLE
250 if (!g_x86DetectionDone)
251 DetectX86Features();
252 return g_hasADX;
253 #else
254 return false;
255 #endif
256 }
257
258 /// \brief Determine AVX availability
259 /// \return true if AVX is determined to be available, false otherwise
260 /// \details HasAVX() is a runtime check performed using CPUID
261 /// \since Crypto++ 8.0
262 /// \note This function is only available on Intel IA-32 platforms
263 inline bool HasAVX()
264 {
265 #if CRYPTOPP_AVX_AVAILABLE
266 if (!g_x86DetectionDone)
267 DetectX86Features();
268 return g_hasAVX;
269 #else
270 return false;
271 #endif
272 }
273
274 /// \brief Determine AVX2 availability
275 /// \return true if AVX2 is determined to be available, false otherwise
276 /// \details HasAVX2() is a runtime check performed using CPUID
277 /// \since Crypto++ 8.0
278 /// \note This function is only available on Intel IA-32 platforms
279 inline bool HasAVX2()
280 {
281 #if CRYPTOPP_AVX2_AVAILABLE
282 if (!g_x86DetectionDone)
283 DetectX86Features();
284 return g_hasAVX2;
285 #else
286 return false;
287 #endif
288 }
289
290 /// \brief Determine RDRAND availability
291 /// \return true if RDRAND is determined to be available, false otherwise
292 /// \details HasRDRAND() is a runtime check performed using CPUID
293 /// \note This function is only available on Intel IA-32 platforms
294 inline bool HasRDRAND()
295 {
296 #if CRYPTOPP_RDRAND_AVAILABLE
297 if (!g_x86DetectionDone)
298 DetectX86Features();
299 return g_hasRDRAND;
300 #else
301 return false;
302 #endif
303 }
304
305 /// \brief Determine RDSEED availability
306 /// \return true if RDSEED is determined to be available, false otherwise
307 /// \details HasRDSEED() is a runtime check performed using CPUID
308 /// \note This function is only available on Intel IA-32 platforms
309 inline bool HasRDSEED()
310 {
311 #if CRYPTOPP_RDSEED_AVAILABLE
312 if (!g_x86DetectionDone)
313 DetectX86Features();
314 return g_hasRDSEED;
315 #else
316 return false;
317 #endif
318 }
319
320 /// \brief Determine Padlock RNG availability
321 /// \return true if VIA Padlock RNG is determined to be available, false otherwise
322 /// \details HasPadlockRNG() is a runtime check performed using CPUID
323 /// \note This function is only available on Intel IA-32 platforms
324 inline bool HasPadlockRNG()
325 {
326 #if CRYPTOPP_PADLOCK_RNG_AVAILABLE
327 if (!g_x86DetectionDone)
328 DetectX86Features();
329 return g_hasPadlockRNG;
330 #else
331 return false;
332 #endif
333 }
334
335 /// \brief Determine Padlock ACE availability
336 /// \return true if VIA Padlock ACE is determined to be available, false otherwise
337 /// \details HasPadlockACE() is a runtime check performed using CPUID
338 /// \note This function is only available on Intel IA-32 platforms
339 inline bool HasPadlockACE()
340 {
341 #if CRYPTOPP_PADLOCK_ACE_AVAILABLE
342 if (!g_x86DetectionDone)
343 DetectX86Features();
344 return g_hasPadlockACE;
345 #else
346 return false;
347 #endif
348 }
349
350 /// \brief Determine Padlock ACE2 availability
351 /// \return true if VIA Padlock ACE2 is determined to be available, false otherwise
352 /// \details HasPadlockACE2() is a runtime check performed using CPUID
353 /// \note This function is only available on Intel IA-32 platforms
354 inline bool HasPadlockACE2()
355 {
356 #if CRYPTOPP_PADLOCK_ACE2_AVAILABLE
357 if (!g_x86DetectionDone)
358 DetectX86Features();
359 return g_hasPadlockACE2;
360 #else
361 return false;
362 #endif
363 }
364
365 /// \brief Determine Padlock PHE availability
366 /// \return true if VIA Padlock PHE is determined to be available, false otherwise
367 /// \details HasPadlockPHE() is a runtime check performed using CPUID
368 /// \note This function is only available on Intel IA-32 platforms
369 inline bool HasPadlockPHE()
370 {
371 #if CRYPTOPP_PADLOCK_PHE_AVAILABLE
372 if (!g_x86DetectionDone)
373 DetectX86Features();
374 return g_hasPadlockPHE;
375 #else
376 return false;
377 #endif
378 }
379
380 /// \brief Determine Padlock PMM availability
381 /// \return true if VIA Padlock PMM is determined to be available, false otherwise
382 /// \details HasPadlockPMM() is a runtime check performed using CPUID
383 /// \note This function is only available on Intel IA-32 platforms
384 inline bool HasPadlockPMM()
385 {
386 #if CRYPTOPP_PADLOCK_PMM_AVAILABLE
387 if (!g_x86DetectionDone)
388 DetectX86Features();
389 return g_hasPadlockPMM;
390 #else
391 return false;
392 #endif
393 }
394
395 /// \brief Determine if the CPU is an Intel P4
396 /// \return true if the CPU is a P4, false otherwise
397 /// \details IsP4() is a runtime check performed using CPUID
398 /// \note This function is only available on Intel IA-32 platforms
399 inline bool IsP4()
400 {
401 if (!g_x86DetectionDone)
402 DetectX86Features();
403 return g_isP4;
404 }
405
406 /// \brief Provides the cache line size
407 /// \return lower bound on the size of a cache line in bytes, if available
408 /// \details GetCacheLineSize() returns the lower bound on the size of a cache line, if it
409 /// is available. If the value is not available at runtime, then 32 is returned for a 32-bit
410 /// processor and 64 is returned for a 64-bit processor.
411 /// \details x86/x32/x64 uses CPUID to determine the value and it is usually accurate. PowerPC
412 /// and AIX also makes the value available to user space and it is also usually accurate. The
413 /// ARM processor equivalent is a privileged instruction, so a compile time value is returned.
414 inline int GetCacheLineSize()
415 {
416 if (!g_x86DetectionDone)
417 DetectX86Features();
418 return g_cacheLineSize;
419 }
420 //@}
421
422 #endif // CRYPTOPP_BOOL_X86 || CRYPTOPP_BOOL_X32 || CRYPTOPP_BOOL_X64
423
424 // ***************************** ARM-32, Aarch32 and Aarch64 ***************************** //
425
426 #if CRYPTOPP_BOOL_ARM32 || CRYPTOPP_BOOL_ARMV8 || CRYPTOPP_DOXYGEN_PROCESSING
427
428 // Hide from Doxygen
429 #ifndef CRYPTOPP_DOXYGEN_PROCESSING
430 extern bool g_ArmDetectionDone;
431 extern bool g_hasARMv7;
432 extern bool g_hasNEON;
433 extern bool g_hasPMULL;
434 extern bool g_hasCRC32;
435 extern bool g_hasAES;
436 extern bool g_hasSHA1;
437 extern bool g_hasSHA2;
438 extern bool g_hasSHA512;
439 extern bool g_hasSHA3;
440 extern bool g_hasSM3;
441 extern bool g_hasSM4;
442 void CRYPTOPP_API DetectArmFeatures();
443 #endif // CRYPTOPP_DOXYGEN_PROCESSING
444
445 /// \name ARM A-32, Aarch32 and AArch64 CPU FEATURES
446 //@{
447
448 /// \brief Determine if an ARM processor is ARMv7 or above
449 /// \return true if the hardware is ARMv7 or above, false otherwise.
450 /// \details Some AES code requires ARMv7 or above
451 /// \since Crypto++ 8.0
452 /// \note This function is only available on ARM-32, Aarch32 and Aarch64 platforms
453 inline bool HasARMv7()
454 {
455 // ASIMD is a core feature on Aarch32 and Aarch64 like SSE2 is a core feature on x86_64
456 #if defined(__aarch32__) || defined(__aarch64__)
457 return true;
458 #else
459 if (!g_ArmDetectionDone)
460 DetectArmFeatures();
461 return g_hasARMv7;
462 #endif
463 }
464
465 /// \brief Determine if an ARM processor has Advanced SIMD available
466 /// \return true if the hardware is capable of Advanced SIMD at runtime, false otherwise.
467 /// \details Advanced SIMD instructions are available under most ARMv7, Aarch32 and Aarch64.
468 /// \details Runtime support requires compile time support. When compiling with GCC, you may
469 /// need to compile with <tt>-mfpu=neon</tt> (32-bit) or <tt>-march=armv8-a</tt>
470 /// (64-bit). Also see ARM's <tt>__ARM_NEON</tt> preprocessor macro.
471 /// \since Crypto++ 5.6.4
472 /// \note This function is only available on ARM-32, Aarch32 and Aarch64 platforms
473 inline bool HasNEON()
474 {
475 // ASIMD is a core feature on Aarch32 and Aarch64 like SSE2 is a core feature on x86_64
476 #if defined(CRYPTOPP_ARM_ASIMD_AVAILABLE)
477 return true;
478 #elif defined(CRYPTOPP_ARM_NEON_AVAILABLE)
479 if (!g_ArmDetectionDone)
480 DetectArmFeatures();
481 return g_hasNEON;
482 #else
483 return false;
484 #endif
485 }
486
487 /// \brief Determine if an ARM processor has CRC32 available
488 /// \return true if the hardware is capable of CRC32 at runtime, false otherwise.
489 /// \details CRC32 instructions provide access to the processor's CRC-32 and CRC-32C
490 /// instructions. They are provided by ARM C Language Extensions 2.0 (ACLE 2.0) and
491 /// available under Aarch32 and Aarch64.
492 /// \details Runtime support requires compile time support. When compiling with GCC,
493 /// you may need to compile with <tt>-march=armv8-a+crc</tt>; while Apple requires
494 /// <tt>-arch arm64</tt>. Also see ARM's <tt>__ARM_FEATURE_CRC32</tt> preprocessor macro.
495 /// \since Crypto++ 5.6.4
496 /// \note This function is only available on Aarch32 and Aarch64 platforms
497 inline bool HasCRC32()
498 {
499 #if defined(CRYPTOPP_ARM_CRC32_AVAILABLE)
500 if (!g_ArmDetectionDone)
501 DetectArmFeatures();
502 return g_hasCRC32;
503 #else
504 return false;
505 #endif
506 }
507
508 /// \brief Determine if an ARM processor has AES available
509 /// \return true if the hardware is capable of AES at runtime, false otherwise.
510 /// \details AES is part of the optional Crypto extensions on Aarch32 and Aarch64. They are
511 /// accessed using ARM C Language Extensions 2.0 (ACLE 2.0).
512 /// \details Runtime support requires compile time support. When compiling with GCC, you may
513 /// need to compile with <tt>-march=armv8-a+crypto</tt>; while Apple requires
514 /// <tt>-arch arm64</tt>. Also see ARM's <tt>__ARM_FEATURE_CRYPTO</tt> preprocessor macro.
515 /// \since Crypto++ 5.6.4
516 /// \note This function is only available on Aarch32 and Aarch64 platforms
517 inline bool HasAES()
518 {
519 #if defined(CRYPTOPP_ARM_AES_AVAILABLE)
520 if (!g_ArmDetectionDone)
521 DetectArmFeatures();
522 return g_hasAES;
523 #else
524 return false;
525 #endif
526 }
527
528 /// \brief Determine if an ARM processor provides Polynomial Multiplication
529 /// \return true if the hardware is capable of polynomial multiplications at runtime,
530 /// false otherwise.
531 /// \details The multiplication instructions are available under Aarch32 and Aarch64.
532 /// \details Runtime support requires compile time support. When compiling with GCC,
533 /// you may need to compile with <tt>-march=armv8-a+crypto</tt>; while Apple requires
534 /// <tt>-arch arm64</tt>. Also see ARM's <tt>__ARM_FEATURE_CRYPTO</tt> preprocessor macro.
535 /// \since Crypto++ 5.6.4
536 /// \note This function is only available on Aarch32 and Aarch64 platforms
537 inline bool HasPMULL()
538 {
539 #if defined(CRYPTOPP_ARM_PMULL_AVAILABLE)
540 if (!g_ArmDetectionDone)
541 DetectArmFeatures();
542 return g_hasPMULL;
543 #else
544 return false;
545 #endif
546 }
547
548 /// \brief Determine if an ARM processor has SHA1 available
549 /// \return true if the hardware is capable of SHA1 at runtime, false otherwise.
550 /// \details SHA1 is part of the optional Crypto extensions on Aarch32 and Aarch64. They are
551 /// accessed using ARM C Language Extensions 2.0 (ACLE 2.0).
552 /// \details Runtime support requires compile time support. When compiling with GCC, you may
553 /// need to compile with <tt>-march=armv8-a+crypto</tt>; while Apple requires
554 /// <tt>-arch arm64</tt>. Also see ARM's <tt>__ARM_FEATURE_CRYPTO</tt> preprocessor macro.
555 /// \since Crypto++ 5.6.4
556 /// \note This function is only available on Aarch32 and Aarch64 platforms
557 inline bool HasSHA1()
558 {
559 #if defined(CRYPTOPP_ARM_SHA1_AVAILABLE)
560 if (!g_ArmDetectionDone)
561 DetectArmFeatures();
562 return g_hasSHA1;
563 #else
564 return false;
565 #endif
566 }
567
568 /// \brief Determine if an ARM processor has SHA256 available
569 /// \return true if the hardware is capable of SHA256 at runtime, false otherwise.
570 /// \details SHA256 is part of the optional Crypto extensions on Aarch32 and Aarch64. They are
571 /// accessed using ARM C Language Extensions 2.0 (ACLE 2.0).
572 /// \details Runtime support requires compile time support. When compiling with GCC, you may
573 /// need to compile with <tt>-march=armv8-a+crypto</tt>; while Apple requires
574 /// <tt>-arch arm64</tt>. Also see ARM's <tt>__ARM_FEATURE_CRYPTO</tt> preprocessor macro.
575 /// \since Crypto++ 5.6.4
576 /// \note This function is only available on Aarch32 and Aarch64 platforms
577 inline bool HasSHA2()
578 {
579 #if defined(CRYPTOPP_ARM_SHA2_AVAILABLE)
580 if (!g_ArmDetectionDone)
581 DetectArmFeatures();
582 return g_hasSHA2;
583 #else
584 return false;
585 #endif
586 }
587
588 /// \brief Determine if an ARM processor has SHA3 available
589 /// \return true if the hardware is capable of SHA3 at runtime, false otherwise.
590 /// \details SHA3 is part of the ARMv8.2 Crypto extensions on Aarch32 and Aarch64. They
591 /// are accessed using ARM C Language Extensions 2.0 (ACLE 2.0).
592 /// \details Runtime support requires compile time support. When compiling with GCC, you
593 /// may need to compile with <tt>-march=armv8.2-a+crypto</tt>; while Apple requires
594 /// <tt>-arch arm64</tt>. Also see ARM's <tt>__ARM_FEATURE_CRYPTO</tt> preprocessor macro.
595 /// \since Crypto++ 8.0
596 /// \note This function is only available on Aarch32 and Aarch64 platforms
597 inline bool HasSHA3()
598 {
599 #if defined(CRYPTOPP_ARM_SHA3_AVAILABLE)
600 if (!g_ArmDetectionDone)
601 DetectArmFeatures();
602 return g_hasSHA3;
603 #else
604 return false;
605 #endif
606 }
607
608 /// \brief Determine if an ARM processor has SHA512 available
609 /// \return true if the hardware is capable of SHA512 at runtime, false otherwise.
610 /// \details SHA512 is part of the ARMv8.2 Crypto extensions on Aarch32 and Aarch64. They
611 /// are accessed using ARM C Language Extensions 2.0 (ACLE 2.0).
612 /// \details Runtime support requires compile time support. When compiling with GCC, you
613 /// may need to compile with <tt>-march=armv8.2-a+crypto</tt>; while Apple requires
614 /// <tt>-arch arm64</tt>. Also see ARM's <tt>__ARM_FEATURE_CRYPTO</tt> preprocessor macro.
615 /// \since Crypto++ 8.0
616 /// \note This function is only available on Aarch32 and Aarch64 platforms
617 inline bool HasSHA512()
618 {
619 #if defined(CRYPTOPP_ARM_SHA512_AVAILABLE)
620 if (!g_ArmDetectionDone)
621 DetectArmFeatures();
622 return g_hasSHA512;
623 #else
624 return false;
625 #endif
626 }
627
628 /// \brief Determine if an ARM processor has SM3 available
629 /// \return true if the hardware is capable of SM3 at runtime, false otherwise.
630 /// \details SM3 is part of the ARMv8.2 Crypto extensions on Aarch32 and Aarch64. They
631 /// are accessed using ARM C Language Extensions 2.0 (ACLE 2.0).
632 /// \details Runtime support requires compile time support. When compiling with GCC, you
633 /// may need to compile with <tt>-march=armv8.2-a+crypto</tt>; while Apple requires
634 /// <tt>-arch arm64</tt>. Also see ARM's <tt>__ARM_FEATURE_CRYPTO</tt> preprocessor macro.
635 /// \since Crypto++ 8.0
636 /// \note This function is only available on Aarch32 and Aarch64 platforms
637 inline bool HasSM3()
638 {
639 #if defined(CRYPTOPP_ARM_SM3_AVAILABLE)
640 if (!g_ArmDetectionDone)
641 DetectArmFeatures();
642 return g_hasSM3;
643 #else
644 return false;
645 #endif
646 }
647
648 /// \brief Determine if an ARM processor has SM4 available
649 /// \return true if the hardware is capable of SM4 at runtime, false otherwise.
650 /// \details SM4 is part of the ARMv8.2 Crypto extensions on Aarch32 and Aarch64. They
651 /// are accessed using ARM C Language Extensions 2.0 (ACLE 2.0).
652 /// \details Runtime support requires compile time support. When compiling with GCC, you
653 /// may need to compile with <tt>-march=armv8.2-a+crypto</tt>; while Apple requires
654 /// <tt>-arch arm64</tt>. Also see ARM's <tt>__ARM_FEATURE_CRYPTO</tt> preprocessor macro.
655 /// \since Crypto++ 8.0
656 /// \note This function is only available on Aarch32 and Aarch64 platforms
657 inline bool HasSM4()
658 {
659 #if defined(CRYPTOPP_ARM_SM4_AVAILABLE)
660 if (!g_ArmDetectionDone)
661 DetectArmFeatures();
662 return g_hasSM4;
663 #else
664 return false;
665 #endif
666 }
667
668 //@}
669
670 #endif // CRYPTOPP_BOOL_ARM32 || CRYPTOPP_BOOL_ARMV8
671
672 // ***************************** PowerPC ***************************** //
673
674 #if CRYPTOPP_BOOL_PPC32 || CRYPTOPP_BOOL_PPC64 || CRYPTOPP_DOXYGEN_PROCESSING
675
676 // Hide from Doxygen
677 #ifndef CRYPTOPP_DOXYGEN_PROCESSING
678 extern bool g_PowerPcDetectionDone;
679 extern bool g_hasAltivec;
680 extern bool g_hasPower7;
681 extern bool g_hasPower8;
682 extern bool g_hasPower9;
683 extern bool g_hasAES;
684 extern bool g_hasPMULL;
685 extern bool g_hasSHA256;
686 extern bool g_hasSHA512;
687 extern bool g_hasDARN;
688 extern word32 g_cacheLineSize;
689 void CRYPTOPP_API DetectPowerPcFeatures();
690 #endif // CRYPTOPP_DOXYGEN_PROCESSING
691
692 /// \name POWERPC CPU FEATURES
693 //@{
694
695 /// \brief Determine if a PowerPC processor has Altivec available
696 /// \return true if the hardware is capable of Altivec at runtime, false otherwise.
697 /// \details Altivec instructions are available on modern PowerPCs.
698 /// \details Runtime support requires compile time support. When compiling with GCC, you may
699 /// need to compile with <tt>-mcpu=power4</tt>; while IBM XL C/C++ compilers require
700 /// <tt>-qarch=pwr6 -qaltivec</tt>. Also see PowerPC's <tt>_ALTIVEC_</tt> preprocessor macro.
701 /// \note This function is only available on PowerPC and PowerPC-64 platforms
702 inline bool HasAltivec()
703 {
704 #if CRYPTOPP_ALTIVEC_AVAILABLE
705 if (!g_PowerPcDetectionDone)
706 DetectPowerPcFeatures();
707 return g_hasAltivec;
708 #else
709 return false;
710 #endif
711 }
712
713 /// \brief Determine if a PowerPC processor has Power7 available
714 /// \return true if the hardware is capable of Power7 at runtime, false otherwise.
715 /// \details Runtime support requires compile time support. When compiling with GCC, you may
716 /// need to compile with <tt>-mcpu=power7</tt>; while IBM XL C/C++ compilers require
717 /// <tt>-qarch=pwr7 -qaltivec</tt>. Also see PowerPC's <tt>_ALTIVEC_</tt> preprocessor macro.
718 /// \note This function is only available on PowerPC and PowerPC-64 platforms
719 inline bool HasPower7()
720 {
721 #if CRYPTOPP_POWER7_AVAILABLE
722 if (!g_PowerPcDetectionDone)
723 DetectPowerPcFeatures();
724 return g_hasPower7;
725 #else
726 return false;
727 #endif
728 }
729
730 /// \brief Determine if a PowerPC processor has Power8 available
731 /// \return true if the hardware is capable of Power8 at runtime, false otherwise.
732 /// \details Runtime support requires compile time support. When compiling with GCC, you may
733 /// need to compile with <tt>-mcpu=power8</tt>; while IBM XL C/C++ compilers require
734 /// <tt>-qarch=pwr8 -qaltivec</tt>. Also see PowerPC's <tt>_ALTIVEC_</tt> preprocessor macro.
735 /// \note This function is only available on PowerPC and PowerPC-64 platforms
736 inline bool HasPower8()
737 {
738 #if CRYPTOPP_POWER8_AVAILABLE
739 if (!g_PowerPcDetectionDone)
740 DetectPowerPcFeatures();
741 return g_hasPower8;
742 #else
743 return false;
744 #endif
745 }
746
747 /// \brief Determine if a PowerPC processor has Power9 available
748 /// \return true if the hardware is capable of Power9 at runtime, false otherwise.
749 /// \details Runtime support requires compile time support. When compiling with GCC, you may
750 /// need to compile with <tt>-mcpu=power9</tt>; while IBM XL C/C++ compilers require
751 /// <tt>-qarch=pwr9 -qaltivec</tt>. Also see PowerPC's <tt>_ALTIVEC_</tt> preprocessor macro.
752 /// \note This function is only available on PowerPC and PowerPC-64 platforms
753 inline bool HasPower9()
754 {
755 #if CRYPTOPP_POWER9_AVAILABLE
756 if (!g_PowerPcDetectionDone)
757 DetectPowerPcFeatures();
758 return g_hasPower9;
759 #else
760 return false;
761 #endif
762 }
763
764 /// \brief Determine if a PowerPC processor has AES available
765 /// \return true if the hardware is capable of AES at runtime, false otherwise.
766 /// \details AES is part of the in-crypto extensions on Power8 and Power9.
767 /// \details Runtime support requires compile time support. When compiling with GCC, you may
768 /// need to compile with <tt>-mcpu=power8</tt>; while IBM XL C/C++ compilers require
769 /// <tt>-qarch=pwr8 -qaltivec</tt>. Also see PowerPC's <tt>__CRYPTO</tt> preprocessor macro.
770 /// \note This function is only available on PowerPC and PowerPC-64 platforms
771 inline bool HasAES()
772 {
773 #if CRYPTOPP_POWER8_AES_AVAILABLE
774 if (!g_PowerPcDetectionDone)
775 DetectPowerPcFeatures();
776 return g_hasAES;
777 #else
778 return false;
779 #endif
780 }
781
782 /// \brief Determine if a PowerPC processor has Polynomial Multiply available
783 /// \return true if the hardware is capable of PMULL at runtime, false otherwise.
784 /// \details PMULL is part of the in-crypto extensions on Power8 and Power9.
785 /// \details Runtime support requires compile time support. When compiling with GCC, you may
786 /// need to compile with <tt>-mcpu=power8</tt>; while IBM XL C/C++ compilers require
787 /// <tt>-qarch=pwr8 -qaltivec</tt>. Also see PowerPC's <tt>__CRYPTO</tt> preprocessor macro.
788 /// \note This function is only available on PowerPC and PowerPC-64 platforms
789 inline bool HasPMULL()
790 {
791 #if CRYPTOPP_POWER8_VMULL_AVAILABLE
792 if (!g_PowerPcDetectionDone)
793 DetectPowerPcFeatures();
794 return g_hasPMULL;
795 #else
796 return false;
797 #endif
798 }
799
800 /// \brief Determine if a PowerPC processor has SHA256 available
801 /// \return true if the hardware is capable of SHA256 at runtime, false otherwise.
802 /// \details SHA is part of the in-crypto extensions on Power8 and Power9.
803 /// \details Runtime support requires compile time support. When compiling with GCC, you may
804 /// need to compile with <tt>-mcpu=power8</tt>; while IBM XL C/C++ compilers require
805 /// <tt>-qarch=pwr8 -qaltivec</tt>. Also see PowerPC's <tt>__CRYPTO</tt> preprocessor macro.
806 /// \note This function is only available on PowerPC and PowerPC-64 platforms
807 inline bool HasSHA256()
808 {
809 #if CRYPTOPP_POWER8_SHA_AVAILABLE
810 if (!g_PowerPcDetectionDone)
811 DetectPowerPcFeatures();
812 return g_hasSHA256;
813 #else
814 return false;
815 #endif
816 }
817
818 /// \brief Determine if a PowerPC processor has SHA512 available
819 /// \return true if the hardware is capable of SHA512 at runtime, false otherwise.
820 /// \details SHA is part of the in-crypto extensions on Power8 and Power9.
821 /// \details Runtime support requires compile time support. When compiling with GCC, you may
822 /// need to compile with <tt>-mcpu=power8</tt>; while IBM XL C/C++ compilers require
823 /// <tt>-qarch=pwr8 -qaltivec</tt>. Also see PowerPC's <tt>__CRYPTO</tt> preprocessor macro.
824 /// \note This function is only available on PowerPC and PowerPC-64 platforms
825 inline bool HasSHA512()
826 {
827 #if CRYPTOPP_POWER8_SHA_AVAILABLE
828 if (!g_PowerPcDetectionDone)
829 DetectPowerPcFeatures();
830 return g_hasSHA512;
831 #else
832 return false;
833 #endif
834 }
835
836 /// \brief Determine if a PowerPC processor has DARN available
837 /// \return true if the hardware is capable of DARN at runtime, false otherwise.
838 /// \details Runtime support requires compile time support. When compiling with GCC, you may
839 /// need to compile with <tt>-mcpu=power9</tt>; while IBM XL C/C++ compilers require
840 /// <tt>-qarch=pwr9 -qaltivec</tt>. Also see PowerPC's <tt>_ALTIVEC_</tt> preprocessor macro.
841 /// \note This function is only available on PowerPC and PowerPC-64 platforms
842 inline bool HasDARN()
843 {
844 #if CRYPTOPP_POWER9_AVAILABLE
845 if (!g_PowerPcDetectionDone)
846 DetectPowerPcFeatures();
847 // see comments in cpu.cpp
848 # if defined(__ibmxl__) && defined(__linux__)
849 return false;
850 # else
851 return g_hasDARN;
852 # endif
853 #else
854 return false;
855 #endif
856 }
857
858 /// \brief Provides the cache line size
859 /// \return lower bound on the size of a cache line in bytes, if available
860 /// \details GetCacheLineSize() returns the lower bound on the size of a cache line, if it
861 /// is available. If the value is not available at runtime, then 32 is returned for a 32-bit
862 /// processor and 64 is returned for a 64-bit processor.
863 /// \details x86/x32/x64 uses CPUID to determine the value and it is usually accurate. PowerPC
864 /// and AIX also makes the value available to user space and it is also usually accurate. The
865 /// ARM processor equivalent is a privileged instruction, so a compile time value is returned.
866 inline int GetCacheLineSize()
867 {
868 if (!g_PowerPcDetectionDone)
869 DetectPowerPcFeatures();
870 return g_cacheLineSize;
871 }
872
873 //@}
874
875 #endif // CRYPTOPP_BOOL_PPC32 || CRYPTOPP_BOOL_PPC64
876
877 // ***************************** L1 cache line ***************************** //
878
879 // Non-Intel systems
880 #if !(CRYPTOPP_BOOL_X86 || CRYPTOPP_BOOL_X32 || CRYPTOPP_BOOL_X64 || CRYPTOPP_BOOL_PPC32 || CRYPTOPP_BOOL_PPC64)
881 /// \brief Provides the cache line size
882 /// \return lower bound on the size of a cache line in bytes, if available
883 /// \details GetCacheLineSize() returns the lower bound on the size of a cache line, if it
884 /// is available. If the value is not available at runtime, then 32 is returned for a 32-bit
885 /// processor and 64 is returned for a 64-bit processor.
886 /// \details x86/x32/x64 uses CPUID to determine the value and it is usually accurate. PowerPC
887 /// and AIX also makes the value available to user space and it is also usually accurate. The
888 /// ARM processor equivalent is a privileged instruction, so a compile time value is returned.
889 inline int GetCacheLineSize()
890 {
891 return CRYPTOPP_L1_CACHE_LINE_SIZE;
892 }
893 #endif // Non-Intel systems
894
895 #endif // CRYPTOPP_GENERATE_X64_MASM
896
897 // ***************************** Inline ASM Helper ***************************** //
898
899 #ifndef CRYPTOPP_DOXYGEN_PROCESSING
900
901 #if CRYPTOPP_BOOL_X86 || CRYPTOPP_BOOL_X32 || CRYPTOPP_BOOL_X64
902
903 #ifdef CRYPTOPP_GENERATE_X64_MASM
904 #define AS1(x) x*newline*
905 #define AS2(x, y) x, y*newline*
906 #define AS3(x, y, z) x, y, z*newline*
907 #define ASS(x, y, a, b, c, d) x, y, a*64+b*16+c*4+d*newline*
908 #define ASL(x) label##x:*newline*
909 #define ASJ(x, y, z) x label##y*newline*
910 #define ASC(x, y) x label##y*newline*
911 #define AS_HEX(y) 0##y##h
912 #elif defined(_MSC_VER) || defined(__BORLANDC__)
913 #define AS1(x) __asm {x}
914 #define AS2(x, y) __asm {x, y}
915 #define AS3(x, y, z) __asm {x, y, z}
916 #define ASS(x, y, a, b, c, d) __asm {x, y, (a)*64+(b)*16+(c)*4+(d)}
917 #define ASL(x) __asm {label##x:}
918 #define ASJ(x, y, z) __asm {x label##y}
919 #define ASC(x, y) __asm {x label##y}
920 #define CRYPTOPP_NAKED __declspec(naked)
921 #define AS_HEX(y) 0x##y
922 #else
923 // define these in two steps to allow arguments to be expanded
924 #define GNU_AS1(x) #x ";" NEW_LINE
925 #define GNU_AS2(x, y) #x ", " #y ";" NEW_LINE
926 #define GNU_AS3(x, y, z) #x ", " #y ", " #z ";" NEW_LINE
927 #define GNU_ASL(x) "\n" #x ":" NEW_LINE
928 // clang 5.0.0 and apple clang 9.0.0 don't support numerical backward jumps
929 #if (CRYPTOPP_LLVM_CLANG_VERSION >= 50000) || (CRYPTOPP_APPLE_CLANG_VERSION >= 90000)
930 #define GNU_ASJ(x, y, z) ATT_PREFIX ";" NEW_LINE #x " " #y #z ";" NEW_LINE INTEL_PREFIX ";" NEW_LINE
931 #else
932 #define GNU_ASJ(x, y, z) #x " " #y #z ";" NEW_LINE
933 #endif
934 #define AS1(x) GNU_AS1(x)
935 #define AS2(x, y) GNU_AS2(x, y)
936 #define AS3(x, y, z) GNU_AS3(x, y, z)
937 #define ASS(x, y, a, b, c, d) #x ", " #y ", " #a "*64+" #b "*16+" #c "*4+" #d ";"
938 #define ASL(x) GNU_ASL(x)
939 #define ASJ(x, y, z) GNU_ASJ(x, y, z)
940 #define ASC(x, y) #x " " #y ";"
941 #define CRYPTOPP_NAKED
942 #define AS_HEX(y) 0x##y
943 #endif
944
945 #define IF0(y)
946 #define IF1(y) y
947
948 #ifdef CRYPTOPP_GENERATE_X64_MASM
949 #define ASM_MOD(x, y) ((x) MOD (y))
950 #define XMMWORD_PTR XMMWORD PTR
951 #else
952 // GNU assembler doesn't seem to have mod operator
953 #define ASM_MOD(x, y) ((x)-((x)/(y))*(y))
954 // GAS 2.15 doesn't support XMMWORD PTR. it seems necessary only for MASM
955 #define XMMWORD_PTR
956 #endif
957
958 #if CRYPTOPP_BOOL_X86
959 #define AS_REG_1 ecx
960 #define AS_REG_2 edx
961 #define AS_REG_3 esi
962 #define AS_REG_4 edi
963 #define AS_REG_5 eax
964 #define AS_REG_6 ebx
965 #define AS_REG_7 ebp
966 #define AS_REG_1d ecx
967 #define AS_REG_2d edx
968 #define AS_REG_3d esi
969 #define AS_REG_4d edi
970 #define AS_REG_5d eax
971 #define AS_REG_6d ebx
972 #define AS_REG_7d ebp
973 #define WORD_SZ 4
974 #define WORD_REG(x) e##x
975 #define WORD_PTR DWORD PTR
976 #define AS_PUSH_IF86(x) AS1(push e##x)
977 #define AS_POP_IF86(x) AS1(pop e##x)
978 #define AS_JCXZ jecxz
979 #elif CRYPTOPP_BOOL_X32
980 #define AS_REG_1 ecx
981 #define AS_REG_2 edx
982 #define AS_REG_3 r8d
983 #define AS_REG_4 r9d
984 #define AS_REG_5 eax
985 #define AS_REG_6 r10d
986 #define AS_REG_7 r11d
987 #define AS_REG_1d ecx
988 #define AS_REG_2d edx
989 #define AS_REG_3d r8d
990 #define AS_REG_4d r9d
991 #define AS_REG_5d eax
992 #define AS_REG_6d r10d
993 #define AS_REG_7d r11d
994 #define WORD_SZ 4
995 #define WORD_REG(x) e##x
996 #define WORD_PTR DWORD PTR
997 #define AS_PUSH_IF86(x) AS1(push r##x)
998 #define AS_POP_IF86(x) AS1(pop r##x)
999 #define AS_JCXZ jecxz
1000 #elif CRYPTOPP_BOOL_X64
1001 #ifdef CRYPTOPP_GENERATE_X64_MASM
1002 #define AS_REG_1 rcx
1003 #define AS_REG_2 rdx
1004 #define AS_REG_3 r8
1005 #define AS_REG_4 r9
1006 #define AS_REG_5 rax
1007 #define AS_REG_6 r10
1008 #define AS_REG_7 r11
1009 #define AS_REG_1d ecx
1010 #define AS_REG_2d edx
1011 #define AS_REG_3d r8d
1012 #define AS_REG_4d r9d
1013 #define AS_REG_5d eax
1014 #define AS_REG_6d r10d
1015 #define AS_REG_7d r11d
1016 #else
1017 #define AS_REG_1 rdi
1018 #define AS_REG_2 rsi
1019 #define AS_REG_3 rdx
1020 #define AS_REG_4 rcx
1021 #define AS_REG_5 r8
1022 #define AS_REG_6 r9
1023 #define AS_REG_7 r10
1024 #define AS_REG_1d edi
1025 #define AS_REG_2d esi
1026 #define AS_REG_3d edx
1027 #define AS_REG_4d ecx
1028 #define AS_REG_5d r8d
1029 #define AS_REG_6d r9d
1030 #define AS_REG_7d r10d
1031 #endif
1032 #define WORD_SZ 8
1033 #define WORD_REG(x) r##x
1034 #define WORD_PTR QWORD PTR
1035 #define AS_PUSH_IF86(x)
1036 #define AS_POP_IF86(x)
1037 #define AS_JCXZ jrcxz
1038 #endif
1039
1040 // helper macro for stream cipher output
1041 #define AS_XMM_OUTPUT4(labelPrefix, inputPtr, outputPtr, x0, x1, x2, x3, t, p0, p1, p2, p3, increment)\
1042 AS2( test inputPtr, inputPtr)\
1043 ASC( jz, labelPrefix##3)\
1044 AS2( test inputPtr, 15)\
1045 ASC( jnz, labelPrefix##7)\
1046 AS2( pxor xmm##x0, [inputPtr+p0*16])\
1047 AS2( pxor xmm##x1, [inputPtr+p1*16])\
1048 AS2( pxor xmm##x2, [inputPtr+p2*16])\
1049 AS2( pxor xmm##x3, [inputPtr+p3*16])\
1050 AS2( add inputPtr, increment*16)\
1051 ASC( jmp, labelPrefix##3)\
1052 ASL(labelPrefix##7)\
1053 AS2( movdqu xmm##t, [inputPtr+p0*16])\
1054 AS2( pxor xmm##x0, xmm##t)\
1055 AS2( movdqu xmm##t, [inputPtr+p1*16])\
1056 AS2( pxor xmm##x1, xmm##t)\
1057 AS2( movdqu xmm##t, [inputPtr+p2*16])\
1058 AS2( pxor xmm##x2, xmm##t)\
1059 AS2( movdqu xmm##t, [inputPtr+p3*16])\
1060 AS2( pxor xmm##x3, xmm##t)\
1061 AS2( add inputPtr, increment*16)\
1062 ASL(labelPrefix##3)\
1063 AS2( test outputPtr, 15)\
1064 ASC( jnz, labelPrefix##8)\
1065 AS2( movdqa [outputPtr+p0*16], xmm##x0)\
1066 AS2( movdqa [outputPtr+p1*16], xmm##x1)\
1067 AS2( movdqa [outputPtr+p2*16], xmm##x2)\
1068 AS2( movdqa [outputPtr+p3*16], xmm##x3)\
1069 ASC( jmp, labelPrefix##9)\
1070 ASL(labelPrefix##8)\
1071 AS2( movdqu [outputPtr+p0*16], xmm##x0)\
1072 AS2( movdqu [outputPtr+p1*16], xmm##x1)\
1073 AS2( movdqu [outputPtr+p2*16], xmm##x2)\
1074 AS2( movdqu [outputPtr+p3*16], xmm##x3)\
1075 ASL(labelPrefix##9)\
1076 AS2( add outputPtr, increment*16)
1077
1078 #endif // CRYPTOPP_BOOL_X86 || CRYPTOPP_BOOL_X32 || CRYPTOPP_BOOL_X64
1079
1080 #endif // Not CRYPTOPP_DOXYGEN_PROCESSING
1081
1082 NAMESPACE_END
1083
1084 // Issue 340
1085 #if CRYPTOPP_GCC_DIAGNOSTIC_AVAILABLE
1086 # pragma GCC diagnostic pop
1087 #endif
1088
1089 #endif // CRYPTOPP_CPU_H
config.h
Library configuration file.
CRYPTOPP_L1_CACHE_LINE_SIZE
#define CRYPTOPP_L1_CACHE_LINE_SIZE
L1 data cache line size.
Definition: config_cpu.h:147
CRYPTOPP_API
#define CRYPTOPP_API
Win32 calling convention.
Definition: config_dll.h:119
word32
unsigned int word32
32-bit unsigned datatype
Definition: config_int.h:72
CryptoPP
Crypto++ library namespace.